                                        April 12, 1965

MEMORANDUM TO:  Users of 1401 Autocoder System

SUBJECT:        1401 Autocoder System, Program #1401-AU-037,
                Version 3, Modification Level 10

This modification letter has been prepared for distribution to all
users of the 1401 Autocoder System and contains changes to
Version 3, Modification Level 9 of that system.  These change cards,
enclosed, listed and identified below (Attachment #1) are to be
inserted in the system deck as follows:

Card Number (Cols. 72-75)        Place between cards in system deck
-------------------------        ----------------------------------

C101-C104                        0115-0116
C105-C106                        C090-0176
C107                             C037-0969

Cards C101-106 provide for better noise checking in Pass 1.

Card C107 insures proper assignment of addresses following blank
ORG’s when an iteration takes place.

The following minor restriction or limitation is presently in effect with
regart to the use of 1401 Autocoder when coding macro instructions:

     @’s may not be used in parameters which govern the inclusion of
     entries which are alphameric DC’s, DCW’s, or literals through
     the use of substitution codes of the form )0A through )9I in the
     comments field.

We appreciate your cooperation in making these changes.  A list of the
material distributed with this letter follows:

Users of IBM 1401 Autocoder System                              Page 2
Program #1401-AU-037, Version 3, Modification Level 10

       Item No.                Contents
       -------                 --------

          1                    7 cards (designated C101, C102, etc.)

          2                    Attachment #1 - Listing of Change Cards

          3                    Attachment #2 - Symbolic Changes to
                               Autocoder Listing.

Initial requests for this system which are filled after the date of this
letter will not include the cards itemized above, as there cards are
included in the system deck as corrections.  However, the Autocoder
listing does not include these corrections and should be corrected by the
user by referring to attachment #2.  Any discrepancy between the material
received and the above list, as well as any errors in card reproduction,
should be directed to the attention of the Manager of the Program Information
Department, IBM, 112 East Post Road, White Plains, New York.

This program has been registered by system tape and is listed under the
name and address shown on your order.  Program modifications as and
when made by IBM will be sent to this same address.  Should there be a
change in your system type or in your address, or should you no longer
need maintenance of this particular program, we would appreciate your
notifying your IBM branch office.

Continued reporting of any difficulties encountered in using 1401 Autocoder
will be appreciated.

PROGRAM INFORMATION DEPARTMENT

cc:  FE Managers
     SE Managers

Attachment #1 - Listing of Change Cards
1401 Autocoder System, Program #1401-AU-037 Version 3, Modification Level 10
N0000B759D0’0,                         L014388,380384,388040,0400401040C1013714L

N00000000B759N0000                     L018481,473477,040040,0400401040C1023714L

B601KB759D0’0,                         L014550,542546,550040,0400401040C1033714L

BIP9V13"                               L008781,040040,040040,0400401040C1043714L

N00000000B759N0000                     L018V51,V43V47,040040,0400401040C1053715L

N0000B759N0000                         L014M46,M38M42,040040,0400401040C1063715L

V’64003B                               L008’29,040040,040040,0400401040C1073752L

Attachment #2 - Symbolic Listing Changes

1401 Autocoder System, Program #1401-AU-037 Version 3, Modification Level 8

        Pass/
Action  Page#   Seq.  Pg.  Lin.  Label    Op   Operands
------  -----   ---   ---  ---   -----    --   --------
Change  1/12          5    17             DCW  @N0000@
Change  1/12          5    18             B    NOISE
Change  1/12          5    19             MN   0&X1
Change  1/12          5    20             SW
Change  1/12          5    33             DCW  @N00000000@

Add     1/12          5    341            DCW  @N0000@
Change  1/13          5    49             BEF  EOF
Change  1/13          5    50             B    NOISE
Change  1/13          5    51             MN   0&X1
Change  1/13          5    52             SW
Change  1/14          6    22    NOISE    BCE  4000-21&X2,INPUT&13,"
Change  1/17          6    92             DCW  @N00000000@

Add     1/17          6    931            DCW  @N0000@
Change  1/21          9    19             DCW  @N0000@

Add     1/21          9    201            DCW  @N0000@
Change  5/12          5    82    TSTADD   BWZ  ITER,STADDR,B
Change  5/12          5    88    ITER     ZA   LABADD&X3,NOWCTR