To:	Users
From:	Bob Supnik
Subj:	PDP-1 Simulator Usage
Date:	15-Jan-02

			COPYRIGHT NOTICE

The following copyright notice applies to both the SIMH source and binary:

   Original code published in 1993-2002, written by Robert M Supnik
   Copyright (c) 1993-2002, Robert M Supnik

   Permission is hereby granted, free of charge, to any person obtaining a
   copy of this software and associated documentation files (the "Software"),
   to deal in the Software without restriction, including without limitation
   the rights to use, copy, modify, merge, publish, distribute, sublicense,
   and/or sell copies of the Software, and to permit persons to whom the
   Software is furnished to do so, subject to the following conditions:

   The above copyright notice and this permission notice shall be included in
   all copies or substantial portions of the Software.

   THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
   IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
   FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.  IN NO EVENT SHALL
   ROBERT M SUPNIK BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER
   IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN
   CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.

   Except as contained in this notice, the name of Robert M Supnik shall not
   be used in advertising or otherwise to promote the sale, use or other dealings
   in this Software without prior written authorization from Robert M Supnik.

This memorandum documents the PDP-1 simulator.


1. Simulator Files

sim/		sim_defs.h
		scp.c
		scp_tty.c
		sim_rev.c

sim/pdp1/	pdp1_defs.h
		pdp1_cpu.c
		pdp1_lp.c
		pdp1_stddev.c
		pdp1_sys.c

2. PDP-1 Features

The PDP-1 is configured as follows:

device		simulates
name(s)

CPU		PDP-1 CPU with up to 64KW of memory
PTR,PTP		integral paper tape reader/punch
TTI,TTO		Flexowriter typewriter input/output
LPT		Type 62 line printer

The PDP-1 simulator implements the following unique stop conditions:

	- an unimplemented instruction is decoded, and register
	  STOP_INST is set
	- more than INDMAX indirect addresses are detected during
	  memory reference address decoding
	- more than XCTMAX nested executes are detected during
	  instruction execution
	- wait state entered, and no I/O operations outstanding
	  (ie, no interrupt can ever occur)

The PDP-1 loader supports RIM format tapes.  The DUMP command is not
implemented.

2.1 CPU

The only CPU options are the presence of hardware multiply/divide and the
size of main memory.

	SET CPU MDV		enable multiply/divide
	SET CPU NOMDV		disable multiply/divide
	SET CPU 4K		set memory size = 4K
	SET CPU 8K		set memory size = 8K
	SET CPU 12K		set memory size = 12K
	SET CPU 16K		set memory size = 16K
	SET CPU 20K		set memory size = 20K
	SET CPU 24K		set memory size = 24K
	SET CPU 28K		set memory size = 28K
	SET CPU 32K		set memory size = 32K
	SET CPU 48K		set memory size = 48K
	SET CPU 64K		set memory size = 64K

If memory size is being reduced, and the memory being truncated contains
non-zero data, the simulator asks for confirmation.  Data in the truncated
portion of memory is lost.  Initial memory size is 64K.

CPU registers include the visible state of the processor as well as the
control registers for the interrupt system.

	name		size	comments

	PC		16	program counter
	AC		18	accumulator
	IO		18	IO register
	OV		1	overflow flag
	PF		6	program flags<1:6>
	SS		6	sense switches<1:6>
	TW		18	test word (front panel switches)
	EXTM		1	extend mode
	IOSTA		18	IO status register
	SBON		1	sequence break enable
	SBRQ		1	sequence break request
	SBIP		1	sequence break in progress
	IOH		1	I/O halt in progress
	IOC		1	I/O continue
	PCQ[0:63]	16	PC prior to last jump or interrupt;
				most recent PC change first
	STOP_INST	1	stop on undefined instruction
	SBS_INIT	1	initial state of sequence break enable
	EXTM_INIT	1	initial state of extend mode
	WRU		8	interrupt character

2.2 Programmed I/O Devices

2.2.1 Paper Tape Reader (PTR)

The paper tape reader (PTR) reads data from or a disk file.  The POS
register specifies the number of the next data item to be read.  Thus,
by changing POS, the user can backspace or advance the reader.

The paper tape reader supports the BOOT command.  BOOT PTR copies the
RIM loader into memory and starts it running.

The paper tape reader implements these registers:

	name		size	comments

	BUF		8	last data item processed
	DONE		1	device done flag
	RPLS		1	return restart pulse flag
	POS		31	position in the input file
	TIME		24	time from I/O initiation to interrupt
	STOP_IOE	1	stop on I/O error

Error handling is as follows:

	error	     STOP_IOE	processed as

	not attached	1	report error and stop
			0	out of tape

	end of file	1	report error and stop
			0	out of tape

	OS I/O error	x	report error and stop

2.2.2 Paper Tape Punch (PTP)

The paper tape punch (PTP) writes data to a disk file.  The POS
register specifies the number of the next data item to be written.
Thus, by changing POS, the user can backspace or advance the punch.

The paper tape punch implements these registers:

	name		size	comments

	BUF		8	last data item processed
	DONE		1	device done flag
	RPLS		1	return restart pulse flag
	POS		31	position in the output file
	TIME		24	time from I/O initiation to interrupt
	STOP_IOE	1	stop on I/O error

Error handling is as follows:

	error	     STOP_IOE	processed as

	not attached	1	report error and stop
			0	out of tape

	OS I/O error	x	report error and stop

2.2.3 Terminal Input (TTI)

The terminal input (TTI) polls the console keyboard for input.  It
implements these registers:

	name		size	comments

	BUF		8	last data item processed
	DONE		1	device done flag
	POS		31	number of characters input
	TIME		24	keyboard polling interval

2.2.4 Terminal Output (TTO)

The terminal output (TTO) writes to the simulator console window.
It implements these registers:

	name		size	comments

	BUF		8	last data item processed
	DONE		1	device done flag
	RPLS		1	return restart pulse flag
	POS		31	number of characters output
	TIME		24	time from I/O initiation to interrupt

2.2.5 Type 62 Line Printer (LPT)

The paper line printer (LPT) writes data to a disk file.  The POS
register specifies the number of the next data item to be written.
Thus, by changing POS, the user can backspace or advance the printer.

The line printer implements these registers:

	name		size	comments

	BUF		8	last data item processed
	PNT		1	printing done flag
	SPC		1	spacing done flag
	RPLS		1	return restart pulse flag
	BPTR		6	print buffer pointer
	POS		31	position in the output file
	TIME		24	time from I/O initiation to interrupt
	STOP_IOE	1	stop on I/O error
	LBUF[0:119]	8	line buffer

Error handling is as follows:

	error	     STOP_IOE	processed as

	not attached	1	report error and stop
			0	out of tape or paper

	OS I/O error	x	report error and stop

2.3 Symbolic Display and Input

The PDP-1 simulator implements symbolic display and input.  Display is
controlled by command line switches:

	-a			display as ASCII character
	-c			display as FIODEC character string
	-m			display instruction mnemonics

Input parsing is controlled by the first character typed in or by command
line switches:

	' or -a			ASCII character
	" or -c			three character FIODEC string
	alphabetic		instruction mnemonic
	numeric			octal number

Instruction input uses modified PDP-1 assembler syntax.  There are six
instruction classes: memory reference, shift, skip, operate, IOT, and
LAW.

Memory reference instructions have the format

	memref {I} address

where I signifies indirect reference.  The address is an octal number in
the range 0 - 0177777.

Shift instructions have the format

	shift shift_count

The shift count is an octal number in the range 0-9.

Skip instructions consist of single mnemonics, eg, SZA, SZS4.  Skip
instructions may be or'd together

	skip skip skip...

The sense of a skip can be inverted by including the mnemonic I.

Operate instructions consist of single mnemonics, eg, CLA, CLI.  Operate
instructions may be or'd together

	opr opr opr...

IOT instructions consist of single mnemonics, eg, TYI, TYO.  IOT
instructions may include an octal numeric modifier or the modifier I:

	iot modifier

The simulator does not check the legality of skip, operate, or IOT
combinations.

Finally, the LAW instruction has the format

	LAW {I} immediate

where immediate is in the range 0 to 07777.

2.4 Character Sets

The PDP-1's console was a Frieden Flexowriter; its character encoding
was known as FIODEC.  The PDP-1's line printer used a modified Hollerith
character set.  The following table provides equivalences between ASCII
characters and the PDP-1's I/O devices.  In the console table, UC stands
for upper case.

		 PDP-1			   PDP-1
ASCII		console	 		line printer

000 - 007	none			none
bs		075			none
tab		036			none
012 - 014	none			none
cr		077			none
016 - 037	none			none
space		000	       		000
!		{OR} UC+005		none
"		UC+001			none
#		{IMPLIES} UC+004	none
$		none			none
%		none			none
&		{AND} UC+006		none
'		UC+002			none
(		057			057
)		055			055
*		{TIMES} UC+073		072
+		UC+054			074
,		033			033
-		054			054
.		073			073
/		021			021
0		020			020
1		001			001
2		002			002
3		003			003
4		004			004
5		005			005
6		006			006
7		007			007
8		010			010
9		011			011
:		none			none
;		none			none
<		UC+007			034
=		UC+033			053
>		UC+010			034
?		UC+021			037
@		{MID DOT} 040		{MID DOT} 040
A		UC+061			061
B		UC+062			062
C		UC+063			063
D		UC+064			064
E		UC+065			065
F		UC+066			066
G		UC+067			067
H		UC+070			070
I		UC+071			071
J		UC+041			041
K		UC+042			042
L		UC+043			043
M		UC+044			044
N		UC+045			045
O		UC+046			046
P		UC+047			047
Q		UC+050			050
R		UC+051			051
S		UC+022			022
T		UC+023			023
U		UC+024			024
V		UC+025			025
W		UC+026			026
X		UC+027			027
Y		UC+030			030
Z		UC+031			031
[		UC+057			none
\		{OVERLINE} 056		{OVERLINE} 056
]		UC+055			none
^		{UP ARROW} UC+011	{UP ARROW} 035
_		UC+040			UC+040
`		{RT ARROW} UC+020	036
a		061			none
b		062			none
c		063			none
d		064			none
e		065			none
f		066			none
g		067			none
h		070			none
i		071			none
j		041			none
k		042			none
l		043			none
m		044			none
n		045			none
o		046			none
p		047			none
q		050			none
r		051			none
s		022			none
t		023			none
u		024			none
v		025			none
w		026			none
x		027			none
y		030			none
z		031			none
{		none			none
|		UC+056			076
}		none			none
~		UC+003			013
del		075			none
